Configure Serilog for authorization server